Data cable, S/FTP, Category 7A, AWG23
CU 7120 4P 1200 MHz

Data cable for structured premises cabling. 
For the transmission of digital and analogue voice, video and data signals. 
Suitable for all ICT network applications up to class FA applications (1000 MHz) in accordance with EN 50173-1 and ISO/IEC 11801 and for the transmission of broadband signals (such as cable TV) in accordance with IEC 15018. 
Applicable for Power over Ethernet (PoE) / PoE+.

Electrically and mechanically high-quality Cat.7A data cable - exceeds the requirements of ISO/IEC 11801, IEC 61156-5, EN 50173-1 and prEN 50288-9-1. 
Excellent shielding effect due to individually screened pairs and overall copper braid. 
Reduced outer diameter. Compatible with all current connecting hardware in accordance with EN 50173 and ISO/IEC 11801.

Loop resistance at 20˚ C:			134 Ω/km
Mutual capacitance:				44 pF/m
Impedance at 100 MHz:				100 Ω ± 5 Ω
Transfer impedance at 1/10/30 MHz:		< 5/5/8 mΩ/m
Coupling attenuation 
(limit curve of critical state - IEC 61156):		> 85 db
Near end unbalance 
attenuation LCL at 1-600 MHz:			> 40 db
Delay skew:					14 ns/100m
NVP:						76%

Frequency [MHz]	1	4	10	100	250	500	600	862	1000	1200
Attenuation [dB/100 m]	1,8	3,5	5,4	17,7	28	41	46	54	57	64		
NEXT [dB]	103	103	103	103	103	98	96	92	90	85	
PS NEXT [dB]	100	100	100	100	100	95	93	89	87	82	
ACR-N [dB]	101	100	98	85	75	57	50	38	33	21	
PS-ACR-N [dB]	98	97	95	82	72	54	47	35	30	18	
ACR-F [dB]	108	106	104	92	82	69	64	56	53	46	
PS-ACR-F [dB]	105	103	101	89	79	66	61	53	50	43		
Return loss [dB]	26	30	33	33	28	26	25	24	23	20	

Bending radius 		during draw-in:		≥ 60 mm
			permanently installed:	≥ 30 mm
Tensile strength:				≤ 110 N
Crush resistance:				≥ 1000 N/10 cm
Impact resistance:				≥ 10 impacts
Temperature range	during installation:	0° C to + 50° C
			in operation:		-20° C to + 60° C

Standards: 
Zero halogen, no corrosive gases
IEC 60754-1/-2, EN 50267-2-1/-2-2, VDE 0482-267-2-1/-2-2, AREI-RGIE Art.104-SA
Flame propagation
IEC 60332-1/-2, EN 60332-1-2, VDE 0482-332-1-2, AREI-RGIE Art.104-F1
Flame spread
IEC 60332-3-24, EN 60332-3-24, AREI-RGIE Art.104-F2
Smoke density
IEC 61034-1/-2, EN 61034-1/-2 , VDE 0482-1034-1/-2, AREI-RGIE Art.104-SD
PoE
IEEE 802.3at
Reaction to fire (Euroclasses) 
EN 13501-6:  Dca-s2,d2,a1
Cat./Class
Cat 7A / Class FA - limit values as specified by IEC 61156-5, IEC 61156-7 and EN 50288-9-1 guaranteed

Type:			Dätwyler CU 7120 4P 

Article Number:		191466

quantity:		____________ m

material:		____________ €

wage:			____________ €