Phone panel CU 25/4
Phone panel CU 50/4
unshielded, Category 3

Unshielded 19”/1U phone panels for the transmission of digital (ISDN) and analogue voice signals. 
Especially suitable for all Class C applications in accordance with EN 50173-1 and ISO/IEC 11801. 
The patch panels support cables up to 50 pairs (telephone cables). 
A maximum of four wires may be connected to one RJ45 socket.
A termination aid is available as an optional accessory. This consists of two angular sheets that can easily be fixed to the frame or cabinet and make the cable termination more comfortable. 

Housing: 		Metal
Dimensions:		19"/1 U W x D x H = 482 mm x 129 mm x 44 mm
Termination:  		2-pairs to PIN 3-6, 4-5

Cat./Class
better than Cat.3 
Standards
IEC 60603-7 (RJ45 basic standard, unshielded)
ISO/IEC 11801:2002 / Amd.2:2010
EN 50173-1:2011
TIA/EIA 568-B.2-10:2008

Type:			Phone panel CU 25/4 with 25 x RJ45 jacks, Cat.3
			Phone panel CU 50/4 with 50 x RJ45 jacks, Cat.3

Article Number:		418000		25/4, grey
			418002		25/4, black
			418001		50/4, grey
			418003		50/4, black

Quantity:		_____________ 

material:		_____________ €

wage:			_____________ €