RJ45 module, shielded, Category 6/EA
Module KS‐T 1/8 toolless

For the transmission of digital and analogue voice-, video- and data signals. 
The module KS-T exceeds the IEC 60603-7-5 standard´s requirements for Cat.6 connecting hardware up to 250 MHz. It also fulfils all Class EA Channel requirements up to 500 MHz when combined with Cat.7 and Cat.7A data cables. Therefore it is applicable for 10-gigabit Ethernet transmissions in accordance with IEEE 802.3. 
Useable for Power over Ethernet Plus (PoE+) corresponding to IEEE 802.3at.

Solid zinc die casting housing with mounting clip for installation in Keystone panels and outlets. 
Contact spring with phosphor bronze alloy, plated with gold. 
For connecting the wires a wire manager is used in combination with two integrated moveable housing wings for tool-less IDC connections. Only for cutting the wires a plane wire cutter is necessary. The 360° metal shield ensures a durable fully shielded environment. 
Strain relief via cable tie. The module is re-usable. Potential balancing possibility directly at the module when needed. 
With removable black dust shutter. 
Other colours available as accessories sets.

Solid copper wire:			0,50 mm (AWG 24) to 0,65 mm (AWG 22)
Re-connection:	for AWG 22, AWG 23 and AWG 24 when using the same or bigger wire diameter
Stranded copper wire:			CU 7702 flex (AWG 26/7), re-usable once
Diameter over insulation:		0.70 mm to 1.40 mm (1.60 mm)
Temperature range:	storing:			- 40° C to + 70° C
during installation:	- 10° C to + 60° C
	in operation:		- 20° C to + 60° C

Standards:
Cat. / Class
Cat.6A / Class EA	
IEC 60603-7-51 (Cat. 6A shielded, 500 MHz)
IEC 60512-99-001 (PoE+)
ISO/IEC 11801:2002 / Amd. 2:2010 
EN 50173-1:2011 
TIA/EIA 568-B.2-10:2008

Typ:			Dätwyler Modul KS-T 1/8 

Artikelnummer:		418060

Menge:			_____________ 

Material:		_____________ €

Lohn:			_____________ €