RJ45 module, shielded, Category 6A (IEC)
Module MS-K Plus 1/8

For the transmission of digital and analogue voice, video and data signals. 
The module MS-K Plus is specified up to 500 MHz in accordance with the component standard IEC 60 603-7-51. 
In combination with shielded Category 6A, 7 and 7A data cables all applications up to Class EA are applicable, that is including 10GBase-T (IEEE 802.3an). 
Useable for Power over Ethernet Plus (PoE+) in accordance with IEEE 802.3at.

Compact zinc die casting housing. 
Special construction for high packing density in faceplates/outlets (up to 3 modules). 
Tool-less wire termination. 360° braid connection to the strain relief bar. 
Strain relief bar fixed with a cable tie. 
With snap-in mounting in patch panels and faceplates by a special kind of Keystone fitting (180° turned).

Solid copper wire:				0.51 mm (AWG 24) to 0.63 mm (AWG 22)
Stranded copper wire:				dependent on construction
Re-connection frequency:	≤ 10 times when using the same or bigger wire diameter
Diameter over insulation:		0.70 mm to 1.40 mm (1.60 mm)
Temperature range:	storing:			- 40° C to + 70° C
during installation:	- 10° C to + 60° C
	in operation:		- 20° C to + 60° C
Termination:	Pair-configuration in accordance with TIA 568-A and -B, clearly marked with a colour code
Potential balancing:	6.3 mm flat plug connection capability at the module
Mounting possibilities:	Suitable for patch panel MS-K 24x and faceplates MS-K (2 or 3 port)

Standards:
Cat./Class
Cat.6A / Class EA	
IEC 60603-7-51 (Cat.6A shielded, 500 MHz)
IEC 60512-99-001 (PoE+)
ISO/IEC 11801:2002 / Amd.2:2010 
EN 50173-1:2011 
TIA/EIA 568-B.2-10:2008

Type:			Dätwyler RJ45 module MS-K Plus 1/8 Cat.6A (IEC), with colour code TIA
568-A and -B

Article Number:		440005

Quantity:		_____________ 

material:		_____________ €

wage:			_____________ €