UP-K Faceplate 1x, 2x, 3x
flush / duct mounted

Faceplates applicable for the installation of 1 module with Keystone fitting. 
The modules are easily fitted into the faceplates. 
Integrated dust shutters. 
The central plate has a labelling field with transparent cover. 
Delivered without modules.

Suitable for the following Datwyler modules: 
- PS-GG45 7A 4P shielded 
- RJ45 module KS-T Plus 1/8 Cat. 6A shielded 
- RJ45 module KS-TS 1/8 Cat. 6/EA shielded 
- RJ45 module KS-T 1/8 Cat. 6/EA shielded 
- RJ45 module KU-T 1/8 Cat. 6 / Cat. 5e unshielded

Dimensions: 
Mounting plate:			70 x 70 mm
Central plate:			50 x 50 mm
Cover frame:			80 x 80 mm
Colour:				pure white, similar RAL 9010

Type:			UP-K Faceplate for 1, 2, 3 modules with Keystone snap-in fitting, angled

Article Number:		185866, 185867, 185869

Quantity:		_____________ 

material:		_____________ €

wage:			_____________ €