UP Faceplate 2x
flush / duct mounted, straight outlet

German flush-mount standard faceplate. 
The snap-in modules are easily fitted into the faceplate. 
The central plate has a labelling field with transparent cover. 
Easy to assemble. 
Delivered without Keystone modules.

Suitable for the following Datwyler modules: 
- PS-GG45 7A 4P shielded 
- RJ45 module MS-K Plus 1/8 Cat. 6A shielded 
- RJ45 module KS-T Plus 1/8 Cat. 6A shielded 
- RJ45 module KS-TS 1/8 Cat. 6/EA shielded 
- RJ45 module KS-T 1/8 Cat. 6/EA shielded 
- RJ45 module KS-TA 1/8 Cat. 6/EA shielded, 45 degree angled 
- RJ45 module KU-T 1/8 Cat. 6 / Cat. 5e unshielded

Dimensions: 
Central plate:			50 x 50 mm
Cover frame:			80 x 80 mm
Colour:				pure white, similar RAL 9010

Type:			UP Faceplate for 2 RJ45 Keystone modules, straight

Article Number:		185861

Quantity:		_____________ 

material:		_____________ €

wage:			_____________ €