Patch panel KS 24x
for 24 modules with Keystone fitting

Shielded 19”/1U patch panel for up to 24 modules with Keystone fitting. 
Snap-in modules can be easily fitted into the patch panel. 
Unused ports can be covered with blank covers.

For the modules PS-GG45 7A Datwyler recommends the patch panel MGK 24x.
Front panel made of flame retardant compound, UL94V-0 rated, in combination with stainless steel and a cable strain relief. 
<< Front in black, similar to RAL 9005. >>
<< Front in grey,   similar to RAL 7035. >>
Strain relief with tie wrap. Delivery without modules

Suitable for the following Datwyler modules: 
- RJ45 module KS-T Plus 1/8 Cat. 6A shielded 
- RJ45 module KS-TS 1/8 Cat. 6/EA shielded 
- RJ45 module KS-T 1/8 Cat. 6/EA shielded 
- RJ45 module KU-T 1/8 Cat. 6 / Cat. 5e unshielded 
- RJ45 module MS-C6A 1/8 Cat. 6A 180°-K shielded

Type:			Patch panel KS 24x, 19‘‘/1U , for 24x RJ45 Keystone modules, FTP

Article Number:		418019 (black), 418020 (grey)

Quantity:		_____________ 

material:		_____________ €

wage:			_____________ €